## Reconyx Tags

The following tags are extracted from the maker notes of Reconyx Hyperfire cameras such as the HC500, HC600 and PC900.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteVersion | no |
> 1 | FirmwareVersion | no |
> 4 | FirmwareDate | int16u[2] |
> 6 | TriggerMode | string[2] | 'C' = CodeLoc Not Entered 'E' = External Sensor 'M' = Motion Detection 'T' = Time Lapse
> 7 | Sequence | int16u[2] |
> 9 | EventNumber | int16u[2] |
> 11 | DateTimeOriginal | int16u[6] |
> 18 | MoonPhase | int16u |
> 0 = New 1 = New Crescent 2 = First Quarter 3 = Waxing Gibbous |  | 4 = Full 5 = Waning Gibbous 6 = Last Quarter 7 = Old Crescent
> 19 | AmbientTemperatureFahrenheit | int16s |
> 20 | AmbientTemperature | int16s |
> 21 | SerialNumber | undef[30] |
> 36 | Contrast | int16u |
> 37 | Brightness | int16u |
> 38 | Sharpness | int16u |
> 39 | Saturation | int16u |
> 40 | InfraredIlluminator | int16u | 0 = Off 1 = On
> 41 | MotionSensitivity | int16u |
> 42 | BatteryVoltage | int16u |
> 43 | UserLabel | string[22] |

## Reconyx Type2 Tags

Tags extracted from models such as the UltraFire.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 24 | FirmwareVersion | undef[7] |
> 31 | Micro1Version | undef[7] |
> 38 | BootLoaderVersion | undef[7] |
> 45 | Micro2Version | undef[7] |
> 52 | TriggerMode | undef[1] | 'M' = Motion Detection 'P' = Point and Shoot 'T' = Time Lapse
> 53 | Sequence | int8u[2] |
> 55 | EventNumber | int32u |
> 59 | DateTimeOriginal | int8u[7] |
> 66 | DayOfWeek | int8u |
> 0 = Sunday 1 = Monday 2 = Tuesday 3 = Wednesday |  | 4 = Thursday 5 = Friday 6 = Saturday
> 67 | MoonPhase | int8u |
> 0 = New 1 = New Crescent 2 = First Quarter 3 = Waxing Gibbous |  | 4 = Full 5 = Waning Gibbous 6 = Last Quarter 7 = Old Crescent
> 68 | AmbientTemperatureFahrenheit | int16s |
> 70 | AmbientTemperature | int16s |
> 72 | Illumination | int8u | 0 = Off 1 = On
> 73 | BatteryVoltage | int16u |
> 75 | SerialNumber | string[15] |
> 90 | UserLabel | string[21] |

## Reconyx Type3 Tags

Tags extracted from models such as the HF2 PRO.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 16 | FileNumber | int16u |
> 18 | DirectoryNumber | int16u |
> 42 | FirmwareVersion | int16u[3] |
> 48 | FirmwareDate | int16u[2] |
> 52 | TriggerMode | string[2] | 'M' = Motion Detection 'P' = Point and Shoot 'T' = Time Lapse
> 54 | Sequence | int16u[2] |
> 58 | EventNumber | int16u[2] |
> 62 | DateTimeOriginal | int16u[6] |
> 74 | DayOfWeek | int16u |
> 0 = Sunday 1 = Monday 2 = Tuesday 3 = Wednesday |  | 4 = Thursday 5 = Friday 6 = Saturday
> 76 | MoonPhase | int16u |
> 0 = New 1 = New Crescent 2 = First Quarter 3 = Waxing Gibbous |  | 4 = Full 5 = Waning Gibbous 6 = Last Quarter 7 = Old Crescent
> 78 | AmbientTemperatureFahrenheit | int16s |
> 80 | AmbientTemperature | int16s |
> 82 | Contrast | int16u |
> 84 | Brightness | int16u |
> 86 | Sharpness | int16u |
> 88 | Saturation | int16u |
> 90 | Flash | int16u | 0 = Off 1 = On
> 92 | AmbientInfrared | int16u |
> 94 | AmbientLight | int16u |
> 96 | MotionSensitivity | int16u |
> 98 | BatteryVoltage | int16u |
> 100 | BatteryVoltageAvg | int16u |
> 102 | BatteryType | int16u |
> 104 | UserLabel | string[22] |
> 126 | SerialNumber | unicode[15] |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Mar 7, 2019

<-- ExifTool Tag Names